Kanalog 1.0 Hardware

Function | Parameter | Specification
Analog | DAC Outputs ADC Inputs | (8) +/- 10V @ 10ma, recommended load >2Kohm 12 bit - update rate 11.1KHz all 8 channels (8) +/- 10V 100Kohm input Impedance 12 bit - update rate 11.1KHz all 8 channels
Optos | Opto Isolated Outputs Opto Isolated Inputs | (8) Max differential voltage 80V 25ma (8) 3-24V input, internal 10KOhm series resistor
Differential | Differential Input Receivers | (16) ANSI TIA/EIA-422-B, ANSI TIA/EIA-423-B +/-7V common mode range, 200mv sensitivity Internal 470ohm termination
Relay Drivers | N channel FET Switches | (8) 24V @ 1 Amp max Open Drain switches to ground
Digital I/O | GPIO - LVTTL | (8) Outputs Source/Sink 12ma (8) Inputs LVTTL, 3.3V 1µa max
±15V | On-board DC-DC Generator | 2 Watts (70ma each supply)
RS232 | Driver/Receiver | EIA/TIA-232-F
Terminal Strips | Screw Terminals | 112 Pluggable Screw Terminals (7) x 16 pin 5mm pitch
Watchdog | Charge Pump | DSP communication enables (1) Relay Driver, FET Switch 24V @ 1A
Logic Supply | Voltage Typical Current | +5V ±10% 0.5 A
Environment | Operating Temperature Storage Temperature Humidity | 0-40º C 0-40º C 20-90% Relative Humidity, non-condensing
Dimensions | Length Width Height | 8.5 inches (216mm) 7.0 inches (178 mm) 0.75inches (19 mm)
Green | RoHS | Compliant