Konnect 1.3 Hardware

Function | Parameter | Specification
Inputs

Number

Type

VIH

VIL

Input Resistance

Banks

Bank Commons

32 Inputs

Full Opto Isolation

4.75V min On Voltage, 25V max allowed Voltage

2V Max Off Voltage

4K Ohms

4 Banks of 8 Inputs per bank

Common Anode or Cathode

(Inputs activate with + or - voltage relative to Common)

Outputs

Number

Type

Configuration

Max Voltage

Max Current

On Voltage Drop

16 Outputs

Full Opto Isolation

Darlington Transistor

30V

0.25A

0.6V max @ 2ma

0.9V max @ 0.25A

Connectors

JP8 Aux Bus to KFLOP

Input Commons

J2 Power

IN0, IN1, IN2, IN3

OUT0, OUT1, OUT2 OUT3

16 pin Header (IDC 0.1 inch pitch)

4 pin Pluggable Screw Terminal 5mm pitch

4 pin Pluggable Screw Terminal 5mm pitch

8 pin Pluggable Screw Terminal 5mm pitch

8 pin Pluggable Screw Terminal 5mm pitch

Logic Supplies

Voltage VDD5

Max Current

Voltage VDD33

Max Current

Voltage VDD12

Max Current

+5V ±10%

0.4A

+3.3 ±10%

0.2A

(not used internally)

Environment

Operating Temperature
Storage Temperature
Humidity

Lead

0-40º C

0-40º C
20-90% Relative Humidity, non-condensing

Lead Free RoHS

Dimensions

Length

Width

Height

8.0 inches (203mm)

3.5 inches (89mm)

0.75 inches (19mm)