Next: 11.7 G86 Cycle Up: 11. Canned Cycles Previous: 11.5 G84 Cycle Contents Index

# 11.6 G85 Cycle

The G85 cycle is intended for boring or reaming.

0. Preliminary motion, as described above.

1. Move the Z-axis only at the current feed rate to the Z position.

2. Retract the Z-axis at the current feed rate to clear Z. This motion is very similar to g81 except that the tool is retracted from the hole at feedrate rather than rapid.