Table of contents |

# USB Installation

The first time the KMotion board is connected to a computer's USB port this message should be displayed near the Windows™ Task Bar.

Shortly thereafter, the New Hardware Wizard Should appear.

If you haven't already, download and install the complete KMotion Software including drivers available at:

DynoMotion Software Download

Select: "Install from a list or specific location (Advanced)" and click Next

Browse to within the subdirectory where you selected the KMotion Software to be installed to the "USB DRIVER" subdirectory.

(If the software was installed into the default subdirectory, the location would be: C:\KMOTION\USB DRIVER)

Click Next.

If this screen appears select Continue Anyway.

If successful, the above screen should appear. Click Finish.

The KMotion Board is now ready for use. To verify proper USB connection to the KMotion Board, use the Windows™ Start Button to launch the KMotion Application.

At the main tool bar select the "Console" button to Display the Console Screen.

Press the "Send" button to send a blank line to the KMotion Board. The following should be displayed indicating successful communication between the PC and KMotion Board.

KMotion 2.2

Ready

See Also: Trouble Shooting USB Driver