Table of contents |

# Kanalog 1.0 Hardware

Parameter | Specification
--- | ---
Analog
DAC Outputs | (8) +/- 10V @ 10ma, recommended load >2Kohm 12 bit - update rate 11.1KHz all 8 channels
ADC Inputs | (8) +/- 10V 100Kohm input Impedance 12 bit - update rate 11.1KHz all 8 channels
Optos
Opto Isolated Outputs | (8) Max differential voltage 80V 25ma
Opto Isolated Inputs | (8) 3-24V input, internal 10KOhm series resistor
Differential
Differential Input Receivers | (16) ANSI TIA/EIA-422-B, ANSI TIA/EIA-423-B +/-7V common mode range, 200mv sensitivity Internal 470ohm termination
Relay Drivers
N channel FET Switches | (8) 24V @ 1 Amp max Open Drain switches to ground
Digital I/O
GPIO - LVTTL | (8) Outputs Source/Sink 12ma (8) Inputs LVTTL, 3.3V 1µa max
±15V
On-board DC-DC Generator | 2 Watts (70ma each supply)
RS232
Driver/Receiver | EIA/TIA-232-F
Terminal Strips
Screw Terminals | 112 Pluggable Screw Terminals (7) x 16 pin 5mm pitch
Watchdog
Charge Pump | DSP communication enables (1) Relay Driver, FET Switch 24V @ 1A
Logic Supply
Voltage | +5V ±10%
Typical Current | 0.5 A
Environment
Operating Temperature | 0-40º C
Storage Temperature | 0-40º C
Humidity | 20-90% Relative Humidity, non-condensing
Dimensions
Length | 8.5 inches (216 mm)
Width | 7.0 inches (178 mm)
Height | 0.75 inches (19 mm)
Green
RoHS | Compliant