Next: Tool Path Contour Up: 12.2.1 Cutter Radius Compensation Previous: Two Kinds of Contour Contents Index

### Material Edge Contour

When the contour is the edge of the material, the outline of the edge is described in the NC program. For a material edge contour, the value for the diameter in the tool table is the actual value of the diameter of the tool. The value in the table must be positive. The NC code for a material edge contour is the same regardless of the (actual or intended) diameter of the tool.

Example 1 :

Here is an NC program which cuts material away from the outside of the triangle in figure above. In this example, the cutter compensation radius is the actual radius of the tool in use, which is 0.5, The value for the diameter in the tool table is twice the radius, which is 1.0.

`N0010 G41 G1 X2 Y2 (turn compensation on and make entry move)`

`N0020 Y-1 (follow right side of triangle)`

`N0030 X-2 (follow bottom side of triangle)`

`N0040 X2 Y2 (follow hypotenuse of triangle)`

`N0050 G40 (turn compensation off)`

This will result in the tool following a path consisting of an entry move and the path shown on the left going clockwise around the triangle. Notice that the coordinates of the triangle of material appear in the NC code. Notice also that the tool path includes three arcs which are not explicitly programmed; they are generated automatically.

Next: Tool Path Contour Up: 12.2.1 Cutter Radius Compensation Previous: Two Kinds of Contour Contents Index