<
Table of contents |

# USB Installation Trouble Shooting

If properly installed, a DynoMotion KMotion 2.2 Device should appear under Universal Serial Bus controllers within the Device Manager.

If within Control Panel – System - Device Manager – Universal Serial Bus controllers there is an item “USB High Speed Serial Converter”: This is an incorrect driver, perform the following steps to change the driver:

- Right Click – select “Update Driver”
- Select “Install from a specific location (Advanced)”, then
- Next
- Select “Don’t Search I will choose the driver to install”, then
- Next
- Select “Have Disk”
- Browse to within the directory chosen during the KMotion Installation (Default is C:\KMotion) to subdirectory “USB Driver”
- Select file “ftd2xx.inf”
- Select OK
- Within the Hardware Update Wizard select to highlight “DynoMotion KMotion 2.2 Device”, then
- Next
- Select “Continue
- Select Finish

Within Control Panel – System - Device Manager – Universal Serial Bus controllers, there should now be an item “DynoMotion KMotion 2.2 Device”