Table of contents |

# Konnect 1.3 Hardware

Parameter | Specification
--- | ---
Inputs
Number | 32 Inputs
Type | Full Opto Isolation
VIH | 4.75V min On Voltage, 25V max allowed Voltage
VIL | 2V Max Off Voltage
Input Resistance | 4K Ohms
Banks | 4 Banks of 8 Inputs per bank
Bank Commons | Common Anode or Cathode (Inputs activate with + or - voltage relative to Common)
Outputs
Number | 16 Outputs
Type | Full Opto Isolation
Configuration | Darlington Transistor
Max Voltage | 30V
Max Current | 0.25A
On Voltage Drop | 0.6V max @ 2ma 0.9V max @ 0.25A
Connectors
JP8 Aux Bus to KFLOP | 16 pin Header (IDC 0.1 inch pitch)
Input Commons | 4 pin Pluggable Screw Terminal 5mm pitch
J2 Power | 4 pin Pluggable Screw Terminal 5mm pitch
IN0, IN1, IN2, IN3 | 8 pin Pluggable Screw Terminal 5mm pitch
OUT0, OUT1, OUT2 OUT3 | 8 pin Pluggable Screw Terminal 5mm pitch
Logic Supplies
Voltage VDD5 | +5V ±10%
Max Current | 0.4A
Voltage VDD33 | +3.3 ±10%
Max Current | 0.2A
Voltage VDD12 Max Current | (not used internally)
Environment
Operating Temperature | 0-40º C
Storage Temperature | 0-40º C
Humidity | 20-90% Relative Humidity, non-condensing
Lead | Lead Free RoHS
Dimensions
Length | 8.0 inches (203mm)
Width | 3.5 inches (89mm)
Height | 0.75 inches (19mm)