Table of contents |

# Connecting and using 2 KSteps

Connect the RJ45 cable between KFLOP JP5 and KStep #2 JP26. KFLOP's Step/Dir Generators 4-7 will then be connected to KStep #2. Configure as OutputChan0 12-15 to drive in TTL mode as required by KStep.

You will also need to provide power, GND, and Enable to KStep. The simplest method is usually to connect the 4 pins on J6 between the 2 KSteps.

Back to main article.