USB Installation Trouble Shooting

If properly installed, a DynoMotion KMotion 2.2 Device should appear under Universal Serial Bus controllers within the Device Manager.

If within Control Panel – System - Device Manager – Universal Serial Bus controllers

There is an item “USB High Speed Serial Converter”

This is an incorrect driver.

Perform the following steps to change the driver:

Right Click – select “Update Driver”

Select “Install from a specific location (Advanced)” then Next

Select “Don’t Search I will choose the driver to install” then Next

Select “Have Disk”

Browse to within the directory chosen during the KMotion Installation (Default is C:\KMotion) to subdirectory “USB Driver”

Select file “ftd2xx.inf”

Select OK

Within the Hardware Update Wizard select to highlight “DynoMotion KMotion 2.2 Device”

then Next

Select “Continue Anyway”

Select Finish

Within Control Panel – System - Device Manager – Universal Serial Bus controllers

There should now be an item “DynoMotion KMotion 2.2 Device”