Next: 14.1.4 Setting up the Up: 14.1 Remote EMC with Previous: 14.1.2 Initial Tests Contents Index

##
14.1.3 Setting up the Server

A couple of minor changes need to be made to emc.ini in the following two sections :

`; General section -------------------------------`
`[EMC]`
`; Name of NML file to use, default is emc.nml`
`NML_FILE = emc.nml`

`; section for external NML server parameters -----------------`
`[EMCSERVER]`
`; Name of NML server, e.g., emcsvr; if not found then none will run`
`EMCSERVER = emcsvr`

The emc.nml now needs to be set up to allow the remote client GUI to ``connect'':

`P xemc emcCommand REMOTE 192.168.0.2 W 0 10.0 0 10`
`P xemc emcStatus REMOTE 192.168.0.2 R 0 10.0 0 10`
`P xemc emcError REMOTE 192.168.0.2 R 0 10.0 0 10`
`P xemc toolCmd REMOTE 192.168.0.2 W 0 10.0 0 10`
`P xemc toolSts REMOTE 192.168.0.2 R 0 10.0 0 10`

All the other entries can be left as the default 'LOCAL localhost' or 'SHMEM localhost'.